**USB C DRD**

* Choose UART for USBC DRD debugging port

**Camera**

* Choose 4 I2C interfaces for the 4xCSI inputs

**Display**

* Choose 2x I2C interfaces for 2xDSI outputs.
* Maybe connect some GPIO to the DSI0 connector pin 17 and pin 18 as well as DSI1 connector pin 17 and pin 18. Maybe the user can use them for something as the camera connectors have things connected to them.